1) Program Cortus\eval-r3.0.2a\eval-r3.0.2a.tar\eval-r3.0.2a\cortus\vlog\impl\xstart-aps3-eval\fpga1000.mcs into the PROM.

2) Edit .jtag_ini so that the USB cable is being used and the parallel cable is commented out.

3) Copy dpcutil.dll from the Windows system32 directory into the cortus-ide\toolchain\bin directory.